USB device details
Proton PIC18 JA Demo - USB Input Device	

			
File:  \??\USB#VID_0925&PID_1234#8&2d6dc21&0&1#{a5dcbf10-6530-11d2-901f-00c04fb951ed}
	
Driver key name:  {745a17a0-74d3-11d0-b6fe-00a0c90f57da}\0012
	
Device instance ID:  USB\VID_0925&PID_1234\8&2D6DC21&0&1
	
Device hardware ID:  USB\VID_0925&PID_1234&REV_0001
	
Device service:  HidUsb
	
Device friendly name:  
	
Device location:  Port_#0001.Hub_#0006
	
Device physical object name:  \Device\USBPDO-11

	Device descriptor		
			
  USB:  0x0110
	
  Device class:  0x00
	
  Device subclass:  0x00
	
  Device protocol:  0x00
	
  Max packet size:  0x08 (8)
	
  Vendor:  0x0925 (Lakeview Research)
	
  Product ID:  0x1234
	
  Device ID:  0x0001
	
  Manufacturer:  0x01 (Proton)
	
  Product:  0x02 (PIC18 JA Demo)
	
  Serial number ID:  0x00
	
  Number of configurations:  1
	
  Connection status:  Device connected
	
  Current config value:  0x01
	
  Device bus speed:  Full (USB 1.1, 12 Mbit/s)
	
  Device address:  0x07
	
  Open pipes:   2

	    Pipe information		
			
      Endpoint address:  0x01, Output
	
      Transfer type:  Interrupt
	
      Max packet size:  0x0008 (8)
	
      Interval:  0x0A (10)

	    Pipe information 		
			
      Endpoint address:  0x81, Input
	
      Transfer type:  Interrupt
	
      Max packet size:  0x0008 (8)
	
      Interval:  0x0A (10)

	Configuration descriptor		
			
  Total length:  0x0029
	
  Number of interfaces:  1
	
  Configuration value:  0x01
	
  Configuration ID:  0x00
	
  Attributes:  0xC0 (Bus powered, Self powered)
	
  Max power:  0x32 (100 Ma)

	Interface descriptor		
			
  Interface number:  0x00
	
  Alternate setting:  0x00
	
  Num of endpoints:  2

  Interface class:  0x03 (Human Interface Device)
	
  Interface subclass:  0x00 (No Subclass)
	
  Interface protocol:  0x00 (None)
	
  Interface ID:  0x00

	HID descriptor		
			
  HID:  0x0111
	
  Country code:  0x00
	
  Number of descriptors:  0x01

	Endpoint descriptor		
			
  Endpoint address:  0x01, Output
	
  Transfer type:  Interrupt
	
  Max packet size:  0x0008 (8)
	
  Interval:  0x0A (10)

	Endpoint descriptor 		
			
  Endpoint address:  0x81, Input
	
  Transfer type:  Interrupt
	
  Max packet size:  0x0008 (8)
	
  Interval:  0x0A (10)